· Process Voice destination selection

User can select a destination by speech, data goes to the voice recognition system to produce a processed destination, and then pass it to the navigation system to process it then display an output on the user interface.

· Process Manual Destination Selection

User can select a destination by typing, where data is passed immediately to the navigation system to process it then display an output on the user interface.

· Process Location Request

GPS passes a location request to external GPS satellite to get the exact location of the vehicle.

· Process Output display

The process of displaying an output on the screen by the vehicle system.

· Process Speed Request

GPS passes a speed request to the Speed Calculation Processor in order to calculate speed of the vehicle, and then pass it to the navigation system.